UDC 621.432.018.2

Belik S.U. The results of modeling the mechanical losses in gas turbine engine/ S.U. Belik, I.V. Parsadanov // Internal combustion engines. – 2009. – №2. – P. 20-23.

The multifactor model was used for analyzing the me-chanical losses in high speed diesels with superchargers of a different modification. The results of bench test were used to determine the diesel indicator efficiency factor in the range of operating modes. As an example the diagram shows the planes of change in mechanical losses as a function of temperature of cooling liquid and lubricating oil. Il.4. Bibliogr. 6 names.