УДК 621.432

Zhukov V.A. Increase the heat and hydraulic efficiency of heat-changing apparatus in system of internal combustion engine / V.A. Zhukov, E.N. Nikolenko // Internal combustion

engines. – 2010. – № 1. – P. 102-105.

The article is devoted to valuation of possibility to increase

heat and hydraulic efficiency of heat-changing apparatus

in system of internal combustion engines by correction of

cooling water’s composition and properties. Investigation

was conducted for oil-water cooler of diesel engine YMZ-

840. Numerical simulation of process which take place in

heat-changing apparatus and its analyses in form of criterial

equations shows, that changing of cooling water’s properties

by little fellow additives provide for increase of oil-water

cooler’s heat efficiency and bring down hydraulic resistance

of heat-changing apparatus. Tаblе. 1. Il. 2. Bibliog. 12

names.