UDC 621.43.003.

Eroshchenkov S.A., Korogodsky V.A., Kagramanаyn A.A.,

Vasilenko O.V. Agency of an excess-air coefficient and compression ratio on the thermal efficiency of the sparkignition engine // Internal combustion engines. – 2008. – №1.

– P. 15-21.

Methods of definition of thermal efficiency are considered.

The technique of definition of values of thermal efficiency

with a real working body in view of change of a parameter

k from factor of air surplus and temperature is offered.

Values of thermal efficiency depending on loading are defined.

Il.5. Bibliogr. 9 names.