Chainov N.D. Conjugate heat exchange problem used for defining temperature field for the mean speed engine cyl-inder head/ N.D.Chainov, L.L. Miagkov, A.H. Volodin, N.S. Malastovski // Internal combustion engines. – 2009. – №2 – Р.3-7.

Cylinder head temperature field determination problem for ЧН30/38 marine engine has been considered taking into account the conjugate heat exchange in the cooling cavity. The heat transfer mode has been studied and temperature field for different versions of structure design has been measured. Based on the results of research the opinion on efficiency of numerical modeling has been given. Table 1. Il.5 Bibliogr. 15 names.